IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2025-03-31T06:39:59"
Preprocessor: "NORM3D - SCAN2BIM"
Originating system: "NORM3D - SCAN2BIM"
Application: "NORM3D - SCAN2BIM" version "2025" identifier "NORM3D - SCAN2BIM" by Organization "NORM3D - SCAN2BIM"

People and organizations
  Person "contact@norm3d.com" of Organization (no name given)
  Owner history of Person "contact@norm3d.com" of Organization (no name given) | application "NORM3D - SCAN2BIM" version "2025" identifier "NORM3D - SCAN2BIM" by Organization "NORM3D - SCAN2BIM" | change NOCHANGE | created 1743403199 (2025-03-31T06:39:59Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level 1" | elevation -7.11244440078735
        contains 75 elements
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.0700" | object type "Wall" | names: "Wall:0", "Wall:1", "Wall:2" (+10 more) | material: layers "wall_thickness_0.0700" ("Default wall" 0.0700000002980232)
          28 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:5", "Wall:6", "Wall:10" (+25 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.2)
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 800 x 2070mm" | object type "Door : 800 x 2070mm" | names: "Door : 800 x 2070mm : 0" | material: "Door Panel"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.5200" | object type "Wall" | names: "Wall:9" | material: layers "wall_thickness_0.5200" ("Default wall" 0.519999980926514)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 860 x 575mm" | object type "Window : 860 x 575mm" | names: "Window : 860 x 575mm : 0" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 850 x 580mm" | object type "Window : 850 x 580mm" | names: "Window : 850 x 580mm : 1" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 890 x 585mm" | object type "Window : 890 x 585mm" | names: "Window : 890 x 585mm : 2" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 955 x 2035mm" | object type "Door : 955 x 2035mm" | names: "Door : 955 x 2035mm : 1" | material: "Door Panel"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 1565 x 2370mm" | object type "Door : 1565 x 2370mm" | names: "Door : 1565 x 2370mm : 2" | material: "Door Panel"
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:21", "Wall:22", "Wall:48" (+1 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 395 x 1265mm" | object type "Window : 395 x 1265mm" | names: "Window : 395 x 1265mm : 3" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.4700" | object type "Wall" | names: "Wall:24" | material: layers "wall_thickness_0.4700" ("Default wall" 0.469999998807907)
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 970 x 2055mm" | object type "Door : 970 x 2055mm" | names: "Door : 970 x 2055mm : 3" | material: "Door Panel"
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.0800" | object type "Wall" | names: "Wall:26", "Wall:27", "Wall:38" | material: layers "wall_thickness_0.0800" ("Default wall" 0.0799999982118607)
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.5900" | object type "Wall" | names: "Wall:28" | material: layers "wall_thickness_0.5900" ("Default wall" 0.589999973773956)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 750 x 590mm" | object type "Window : 750 x 590mm" | names: "Window : 750 x 590mm : 4" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 890 x 580mm" | object type "Window : 890 x 580mm" | names: "Window : 890 x 580mm : 5" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.1000" | object type "Wall" | names: "Wall:39" | material: layers "wall_thickness_0.1000" ("Default wall" 0.100000001490116)
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 820 x 2220mm" | object type "Door : 820 x 2220mm" | names: "Door : 820 x 2220mm : 4" | material: "Door Panel"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 915 x 2065mm" | object type "Door : 915 x 2065mm" | names: "Door : 915 x 2065mm : 5" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 415 x 910mm" | object type "Window : 415 x 910mm" | names: "Window : 415 x 910mm : 6" | material: "Window Default"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Rectangular Column:590 x 400mm" | object type "Rectangular Column:590 x 400mm" | names: "Rectangular Column:590 x 400mm" | material: "<Unnamed>" | property sets: Pset_ReinforcementBarPitchOfColumn, Pset_QuantityTakeOff, Pset_ColumnCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
        IFCSPACE "Room 001"
        IFCSPACE "Room 002"
        IFCSPACE "Room 003"
        IFCSPACE "Room 004"
        IFCSPACE "Room 005"
        IFCSPACE "Room 006"
        IFCSPACE "Room 007"
        IFCSPACE "Room 008"
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level 2" | elevation -3.49321627616882
        contains 21 elements
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:59", "Wall:61", "Wall:63" (+2 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.0700" | object type "Wall" | names: "Wall:65", "Wall:66", "Wall:69" (+1 more) | material: layers "wall_thickness_0.0700" ("Default wall" 0.0700000002980232)
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 710 x 2080mm" | object type "Door : 710 x 2080mm" | names: "Door : 710 x 2080mm : 6" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 610 x 900mm" | object type "Window : 610 x 900mm" | names: "Window : 610 x 900mm : 7" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:68" | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 595 x 610mm" | object type "Window : 595 x 610mm" | names: "Window : 595 x 610mm : 8" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 705 x 2080mm" | object type "Door : 705 x 2080mm" | names: "Door : 705 x 2080mm : 7" | material: "Door Panel"
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.5300" | object type "Wall" | names: "Wall:71", "Wall:72", "Wall:73" | material: layers "wall_thickness_0.5300" ("Default wall" 0.529999971389771)
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
        IFCSPACE "Room 009"
        IFCSPACE "Room 010"
        IFCSPACE "Room 011"

Types
  IFCWALLTYPE "wall_thickness_0.0700" | STANDARD | 17 occurrences | material: layers "wall_thickness_0.0700" ("Default wall" 0.0700000002980232) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.2000" | STANDARD | 33 occurrences | material: layers "wall_thickness_0.2000" ("Default wall" 0.2) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door : 800 x 2070mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 800 x 2070mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.5200" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.5200" ("Default wall" 0.519999980926514) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 860 x 575mm" | 1 occurrence | material: "Window Default" | property sets: Window : 860 x 575mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 850 x 580mm" | 1 occurrence | material: "Window Default" | property sets: Window : 850 x 580mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 890 x 585mm" | 1 occurrence | material: "Window Default" | property sets: Window : 890 x 585mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 955 x 2035mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 955 x 2035mm, Pset_DoorCommon
  IFCDOORSTYLE "Door : 1565 x 2370mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 1565 x 2370mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.2000" | STANDARD | 5 occurrences | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 395 x 1265mm" | 1 occurrence | material: "Window Default" | property sets: Window : 395 x 1265mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.4700" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.4700" ("Default wall" 0.469999998807907) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door : 970 x 2055mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 970 x 2055mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.0800" | STANDARD | 3 occurrences | material: layers "wall_thickness_0.0800" ("Default wall" 0.0799999982118607) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.5900" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.5900" ("Default wall" 0.589999973773956) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 750 x 590mm" | 1 occurrence | material: "Window Default" | property sets: Window : 750 x 590mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 890 x 580mm" | 1 occurrence | material: "Window Default" | property sets: Window : 890 x 580mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.1000" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.1000" ("Default wall" 0.100000001490116) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door : 820 x 2220mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 820 x 2220mm, Pset_DoorCommon
  IFCDOORSTYLE "Door : 915 x 2065mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 915 x 2065mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 415 x 910mm" | 1 occurrence | material: "Window Default" | property sets: Window : 415 x 910mm, Pset_WindowCommon
  IFCCOLUMNTYPE "Rectangular Column:590 x 400mm" | COLUMN | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ColumnCommon
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCDOORSTYLE "Door : 710 x 2080mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 710 x 2080mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 610 x 900mm" | 1 occurrence | material: "Window Default" | property sets: Window : 610 x 900mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 595 x 610mm" | 1 occurrence | material: "Window Default" | property sets: Window : 595 x 610mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 705 x 2080mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 705 x 2080mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.5300" | STANDARD | 3 occurrences | material: layers "wall_thickness_0.5300" ("Default wall" 0.529999971389771) | property sets: Pset_WallCommon
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon

Property sets
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "wall_thickness_0.0700" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "wall_thickness_0.5200" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCOPENINGELEMENT, 1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.0700" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCOPENINGELEMENT, 1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5200" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOLUMN)
    Reference = "590 x 400mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.4700" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.0800" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5900" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 2 more contents on 2 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "590 x 400mm" (IFCLABEL)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "590 x 400mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor : 100mm" (IFCLABEL)
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 2.4247 [SQUARE_METRE]
    GrossPerimeter = 6.2494 [METRE]
    GrossVolume = 6.5135 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 2.4247 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 16.6229 [SQUARE_METRE]
    GrossPerimeter = 25.5368 [METRE]
    GrossVolume = 44.6544 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 16.6229 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 146.6618 [SQUARE_METRE]
    GrossPerimeter = 83.7022 [METRE]
    GrossVolume = 393.9816 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 146.6618 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 31.4731 [SQUARE_METRE]
    GrossPerimeter = 23.9203 [METRE]
    GrossVolume = 84.547 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 31.4731 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 8.959 [SQUARE_METRE]
    GrossPerimeter = 12.6147 [METRE]
    GrossVolume = 24.0668 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 8.959 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 2.9322 [SQUARE_METRE]
    GrossPerimeter = 7.2011 [METRE]
    GrossVolume = 7.8768 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 2.9322 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 22.3866 [SQUARE_METRE]
    GrossPerimeter = 19.7433 [METRE]
    GrossVolume = 60.1378 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 22.3866 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 3.5498 [SQUARE_METRE]
    GrossPerimeter = 7.6236 [METRE]
    GrossVolume = 9.536 [CUBIC_METRE]
    Height = 2.6863 [METRE]
    NetFloorArea = 3.5498 [SQUARE_METRE]
  BaseQuantities: 3 more contents on 3 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.0700" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.4700" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.0800" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5900" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.1000" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5300" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.0700" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.5200" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.4700" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.0800" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.5900" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.1000" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.5300" (IFCIDENTIFIER)
  Pset_WallCommon: 1 more content on 0 objects not shown
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Door : 800 x 2070mm | predefined | on 2 type objects
  Pset_DoorCommon | properties | on 8 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 860 x 575mm | predefined | on 1 type object
  Pset_WindowCommon | properties | on 9 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 850 x 580mm | predefined | on 1 type object
  Window : 890 x 585mm | predefined | on 1 type object
  Door : 955 x 2035mm | predefined | on 2 type objects
  Door : 1565 x 2370mm | predefined | on 2 type objects
  Window : 395 x 1265mm | predefined | on 1 type object
  Door : 970 x 2055mm | predefined | on 2 type objects
  Window : 750 x 590mm | predefined | on 1 type object
  Window : 890 x 580mm | predefined | on 1 type object
  Door : 820 x 2220mm | predefined | on 2 type objects
  Door : 915 x 2065mm | predefined | on 2 type objects
  Window : 415 x 910mm | predefined | on 1 type object
  Pset_CoveringCommon | properties | on 11 type objects
    TotalThickness = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Door : 710 x 2080mm | predefined | on 2 type objects
  Window : 610 x 900mm | predefined | on 1 type object
  Window : 595 x 610mm | predefined | on 1 type object
  Door : 705 x 2080mm | predefined | on 2 type objects