IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2025-02-19T02:43:09"
Preprocessor: "NORM3D IFC Exporter"
Originating system: "NORM3D IFC Exporter"
Application: "NORM3D IFC Exporter" version "2025" identifier "NORM3D IFC Exporter" by Organization "NORM3D IFC Exporter"

People and organizations
  Person "contact@norm3d.com" of Organization (no name given)
  Owner history of Person "contact@norm3d.com" of Organization (no name given) | application "NORM3D IFC Exporter" version "2025" identifier "NORM3D IFC Exporter" by Organization "NORM3D IFC Exporter" | change NOCHANGE | created 1739932989 (2025-02-19T02:43:09Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level 2" | elevation -79.2126846313477
        contains 6 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:0", "Wall:2", "Wall:3" | material: layers "wall_thickness_0.2000" ("Default wall" 0.2)
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.1900" | object type "Wall" | names: "Wall:4" | material: layers "wall_thickness_0.1900" ("Default wall" 0.189999997615814)
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Beam:4" | object type "Beam" | names: "Beam:4" | material: "Beam default" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level 1" | elevation -81.7791442871094
        contains 103 elements
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.3300" | object type "Wall" | names: "Wall:5", "Wall:6" | material: layers "wall_thickness_0.3300" ("Default wall" 0.330000013113022)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1590 x 1075mm" | object type "Window : 1590 x 1075mm" | names: "Window : 1590 x 1075mm : 0" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 510 x 715mm" | object type "Window : 510 x 715mm" | names: "Window : 510 x 715mm : 1" | material: "Window Default"
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.4500" | object type "Wall" | names: "Wall:8", "Wall:88" | material: layers "wall_thickness_0.4500" ("Default wall" 0.449999988079071)
          25 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:9", "Wall:11", "Wall:12" (+22 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.2)
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.5900" | object type "Wall" | names: "Wall:13" | material: layers "wall_thickness_0.5900" ("Default wall" 0.589999973773956)
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.4700" | object type "Wall" | names: "Wall:14", "Wall:21", "Wall:22" (+3 more) | material: layers "wall_thickness_0.4700" ("Default wall" 0.469999998807907)
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.6200" | object type "Wall" | names: "Wall:15" | material: layers "wall_thickness_0.6200" ("Default wall" 0.620000004768372)
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 755 x 1970mm" | object type "Door : 755 x 1970mm" | names: "Door : 755 x 1970mm : 0" | material: "Door Panel"
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:16", "Wall:17", "Wall:25" (+5 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1300 x 1055mm" | object type "Window : 1300 x 1055mm" | names: "Window : 1300 x 1055mm : 2" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.3900" | object type "Wall" | names: "Wall:18" | material: layers "wall_thickness_0.3900" ("Default wall" 0.389999985694885)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 815 x 735mm" | object type "Window : 815 x 735mm" | names: "Window : 815 x 735mm : 3" | material: "Window Default"
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.3200" | object type "Wall" | names: "Wall:19", "Wall:33" | material: layers "wall_thickness_0.3200" ("Default wall" 0.319999992847443)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1080 x 1660mm" | object type "Window : 1080 x 1660mm" | names: "Window : 1080 x 1660mm : 4" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1105 x 1660mm" | object type "Window : 1105 x 1660mm" | names: "Window : 1105 x 1660mm : 5" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1900 x 1950mm" | object type "Window : 1900 x 1950mm" | names: "Window : 1900 x 1950mm : 6" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1095 x 1605mm" | object type "Window : 1095 x 1605mm" | names: "Window : 1095 x 1605mm : 7" | material: "Window Default"
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2400" | object type "Wall" | names: "Wall:26", "Wall:78" | material: layers "wall_thickness_0.2400" ("Default wall" 0.239999994635582) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 545 x 885mm" | object type "Window : 545 x 885mm" | names: "Window : 545 x 885mm : 8" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.4200" | object type "Wall" | names: "Wall:38" | material: layers "wall_thickness_0.4200" ("Default wall" 0.419999986886978)
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.0700" | object type "Wall" | names: "Wall:41", "Wall:42", "Wall:74" (+1 more) | material: layers "wall_thickness_0.0700" ("Default wall" 0.0700000002980232)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 395 x 355mm" | object type "Window : 395 x 355mm" | names: "Window : 395 x 355mm : 9" | material: "Window Default"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.0800" | object type "Wall" | names: "Wall:46" | material: layers "wall_thickness_0.0800" ("Default wall" 0.0799999982118607)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 740 x 635mm" | object type "Window : 740 x 635mm" | names: "Window : 740 x 635mm : 10" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 380 x 695mm" | object type "Window : 380 x 695mm" | names: "Window : 380 x 695mm : 11" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 890 x 2070mm" | object type "Door : 890 x 2070mm" | names: "Door : 890 x 2070mm : 1" | material: "Door Panel"
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.3400" | object type "Wall" | names: "Wall:59" | material: layers "wall_thickness_0.3400" ("Default wall" 0.340000003576279)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 590 x 785mm" | object type "Window : 590 x 785mm" | names: "Window : 590 x 785mm : 12" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 810 x 2070mm" | object type "Door : 810 x 2070mm" | names: "Door : 810 x 2070mm : 2" | material: "Door Panel"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 690 x 2060mm" | object type "Door : 690 x 2060mm" | names: "Door : 690 x 2060mm : 3" | material: "Door Panel"
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2700" | object type "Wall" | names: "Wall:68", "Wall:69", "Wall:70" | material: layers "wall_thickness_0.2700" ("Default wall" 0.270000010728836)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 780 x 615mm" | object type "Window : 780 x 615mm" | names: "Window : 780 x 615mm : 13" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 770 x 2070mm" | object type "Door : 770 x 2070mm" | names: "Door : 770 x 2070mm : 4" | material: "Door Panel"
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.3500" | object type "Wall" | names: "Wall:73", "Wall:82" | material: layers "wall_thickness_0.3500" ("Default wall" 0.349999994039536)
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 1430 x 905mm" | object type "Window : 1430 x 905mm" | names: "Window : 1430 x 905mm : 14" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 775 x 2030mm" | object type "Door : 775 x 2030mm" | names: "Door : 775 x 2030mm : 5" | material: "Door Panel"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 1140 x 2295mm" | object type "Door : 1140 x 2295mm" | names: "Door : 1140 x 2295mm : 6" | material: "Door Panel"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Beam:2" | object type "Beam" | names: "Beam:2" | material: "Beam default" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
        IFCSPACE "Room 001"
        IFCSPACE "Room 002"
        IFCSPACE "Room 003"
        IFCSPACE "Room 004"
        IFCSPACE "Room 005"
        IFCSPACE "Room 006"
        IFCSPACE "Room 007"
        IFCSPACE "Room 008"
        IFCSPACE "Room 009"
        IFCSPACE "Room 010"
        IFCSPACE "Room 011"
        IFCSPACE "Room 012"
        IFCSPACE "Room 013"
        IFCSPACE "Room 014"
        IFCSPACE "Room 015"
        IFCSPACE "Room 016"

Types
  IFCWALLTYPE "wall_thickness_0.2000" | STANDARD | 28 occurrences | material: layers "wall_thickness_0.2000" ("Default wall" 0.2) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.1900" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.1900" ("Default wall" 0.189999997615814) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Beam:4" | 1 occurrence
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCWALLTYPE "wall_thickness_0.3300" | STANDARD | 2 occurrences | material: layers "wall_thickness_0.3300" ("Default wall" 0.330000013113022) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 1590 x 1075mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1590 x 1075mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 510 x 715mm" | 1 occurrence | material: "Window Default" | property sets: Window : 510 x 715mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.4500" | STANDARD | 2 occurrences | material: layers "wall_thickness_0.4500" ("Default wall" 0.449999988079071) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.5900" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.5900" ("Default wall" 0.589999973773956) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.4700" | STANDARD | 6 occurrences | material: layers "wall_thickness_0.4700" ("Default wall" 0.469999998807907) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.6200" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.6200" ("Default wall" 0.620000004768372) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door : 755 x 1970mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 755 x 1970mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.2000" | STANDARD | 8 occurrences | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 1300 x 1055mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1300 x 1055mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.3900" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.3900" ("Default wall" 0.389999985694885) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 815 x 735mm" | 1 occurrence | material: "Window Default" | property sets: Window : 815 x 735mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.3200" | STANDARD | 2 occurrences | material: layers "wall_thickness_0.3200" ("Default wall" 0.319999992847443) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 1080 x 1660mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1080 x 1660mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 1105 x 1660mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1105 x 1660mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 1900 x 1950mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1900 x 1950mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 1095 x 1605mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1095 x 1605mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.2400" | STANDARD | 2 occurrences | material: layers "wall_thickness_0.2400" ("Default wall" 0.239999994635582) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 545 x 885mm" | 1 occurrence | material: "Window Default" | property sets: Window : 545 x 885mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.4200" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.4200" ("Default wall" 0.419999986886978) | property sets: Pset_WallCommon
  IFCWALLTYPE "wall_thickness_0.0700" | STANDARD | 4 occurrences | material: layers "wall_thickness_0.0700" ("Default wall" 0.0700000002980232) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 395 x 355mm" | 1 occurrence | material: "Window Default" | property sets: Window : 395 x 355mm, Pset_WindowCommon
  IFCWALLTYPE "wall_thickness_0.0800" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.0800" ("Default wall" 0.0799999982118607) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 740 x 635mm" | 1 occurrence | material: "Window Default" | property sets: Window : 740 x 635mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 380 x 695mm" | 1 occurrence | material: "Window Default" | property sets: Window : 380 x 695mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 890 x 2070mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 890 x 2070mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.3400" | STANDARD | 1 occurrence | material: layers "wall_thickness_0.3400" ("Default wall" 0.340000003576279) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 590 x 785mm" | 1 occurrence | material: "Window Default" | property sets: Window : 590 x 785mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 810 x 2070mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 810 x 2070mm, Pset_DoorCommon
  IFCDOORSTYLE "Door : 690 x 2060mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 690 x 2060mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.2700" | STANDARD | 3 occurrences | material: layers "wall_thickness_0.2700" ("Default wall" 0.270000010728836) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 780 x 615mm" | 1 occurrence | material: "Window Default" | property sets: Window : 780 x 615mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 770 x 2070mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 770 x 2070mm, Pset_DoorCommon
  IFCWALLTYPE "wall_thickness_0.3500" | STANDARD | 2 occurrences | material: layers "wall_thickness_0.3500" ("Default wall" 0.349999994039536) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 1430 x 905mm" | 1 occurrence | material: "Window Default" | property sets: Window : 1430 x 905mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 775 x 2030mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 775 x 2030mm, Pset_DoorCommon
  IFCDOORSTYLE "Door : 1140 x 2295mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 1140 x 2295mm, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "Beam:2" | 1 occurrence
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon

Property sets
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Reference = "Floor : 100mm" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCSLAB)
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCOPENINGELEMENT, 1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2400" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCOPENINGELEMENT, 1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2700" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.1900" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.3300" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.4500" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5900" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 11 more contents on 11 objects not shown
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "wall_thickness_0.2400" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "wall_thickness_0.2700" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 1.617 [SQUARE_METRE]
    GrossPerimeter = 6.3274 [METRE]
    GrossVolume = 3.9038 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 1.617 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 2.8121 [SQUARE_METRE]
    GrossPerimeter = 7.409 [METRE]
    GrossVolume = 6.7892 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 2.8121 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 2.7401 [SQUARE_METRE]
    GrossPerimeter = 7.7757 [METRE]
    GrossVolume = 6.6154 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 2.7401 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 0.1003 [SQUARE_METRE]
    GrossPerimeter = 5.5906 [METRE]
    GrossVolume = 0.2421 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 0.1003 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 1.907 [SQUARE_METRE]
    GrossPerimeter = 6.04 [METRE]
    GrossVolume = 4.6039 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 1.907 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 0.902 [SQUARE_METRE]
    GrossPerimeter = 4.4165 [METRE]
    GrossVolume = 2.1776 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 0.902 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 0.0205 [SQUARE_METRE]
    GrossPerimeter = 5.2743 [METRE]
    GrossVolume = 0.0496 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 0.0205 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 6.0556 [SQUARE_METRE]
    GrossPerimeter = 11.131 [METRE]
    GrossVolume = 14.6198 [CUBIC_METRE]
    Height = 2.4143 [METRE]
    NetFloorArea = 6.0556 [SQUARE_METRE]
  BaseQuantities: 8 more contents on 8 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.1900" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.3300" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.4500" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.5900" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.4700" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.6200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.3900" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 8 more contents on 8 objects not shown
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.1900" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.3300" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.4500" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.5900" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.4700" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.6200" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.3900" (IFCIDENTIFIER)
  Pset_WallCommon: 9 more contents on 8 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Beam:4" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Beam:2" (IFCIDENTIFIER)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.617996215820312 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Height = 0.46000000834465 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.617996215820312 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.680000305175781 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Height = 0.519999980926514 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.680000305175781 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Window : 1590 x 1075mm | predefined | on 1 type object
  Pset_WindowCommon | properties | on 15 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 510 x 715mm | predefined | on 1 type object
  Door : 755 x 1970mm | predefined | on 2 type objects
  Pset_DoorCommon | properties | on 7 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 1300 x 1055mm | predefined | on 1 type object
  Window : 815 x 735mm | predefined | on 1 type object
  Window : 1080 x 1660mm | predefined | on 1 type object
  Window : 1105 x 1660mm | predefined | on 1 type object
  Window : 1900 x 1950mm | predefined | on 1 type object
  Window : 1095 x 1605mm | predefined | on 1 type object
  Window : 545 x 885mm | predefined | on 1 type object
  Window : 395 x 355mm | predefined | on 1 type object
  Window : 740 x 635mm | predefined | on 1 type object
  Window : 380 x 695mm | predefined | on 1 type object
  Door : 890 x 2070mm | predefined | on 2 type objects
  Window : 590 x 785mm | predefined | on 1 type object
  Door : 810 x 2070mm | predefined | on 2 type objects
  Door : 690 x 2060mm | predefined | on 2 type objects
  Window : 780 x 615mm | predefined | on 1 type object
  Door : 770 x 2070mm | predefined | on 2 type objects
  Window : 1430 x 905mm | predefined | on 1 type object
  Door : 775 x 2030mm | predefined | on 2 type objects
  Door : 1140 x 2295mm | predefined | on 2 type objects
  Pset_CoveringCommon | properties | on 16 type objects
    TotalThickness = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]